Charged Particle Tracking

Carnegie Mellon University, (Los Alamos)

Optimize the design of the tracking elements - minimize channels - minimize number of detector types Prototyping Needed.

- resolution and alignment issues. - dE/dx capability needed for PID

Start Counter/ Vertex Chamber

Old Dominion Univ., Florida International Univ.

Based on the D0 (Fermilab) Vertex Detector - In contact with Fermilab people. - Try to initially use D0 rejects + prototypes Critical to optimize the design to Hall D Technology could be used in RadPhi, CLAS - "...will require serious R&D effort."