380 385 390 395 400 405 -15

-10

-5

0 Cost optimization approach comparison around h,b=-12,-9 (w=-6)

Current in 1.8T regime (A)

Cost reduction (k$)

13, 9.75

12.5, 9.375

12, 9

-(h,b) coordinate pairs along descent shown

t=-3

t=-6 t-parameter adjustment h,b steepest descent