Board Information Report
Filename     : C:\Documents and Settings\jonesrt\My Documents\Analog Board, Spring 2009\Amplifier Board.PcbDoc
Date         : 6/25/2009
Time         : 1:39:32 PM
Time Elapsed : 00:00:00

General
    Board Size, 6000milsx2640mils
    Components on board, 884
count : 2

Routing Information
    Routing completion, 100.00%
    Connections, 1513
    Connections routed, 1513
    Connections remaing, 0
count : 4

Layer, Arcs, Pads, Vias, Tracks, Texts, Fills, Regions, ComponentBodies
    Top Layer, 0, 1871, 0, 4647, 0, 0, 0, 0
    GND, 0, 0, 0, 4, 0, 0, 0, 0
    VCC, 0, 0, 0, 4, 0, 0, 0, 0
    BASES, 0, 0, 0, 0, 0, 0, 2, 0
    GND, 0, 0, 0, 4, 0, 0, 0, 0
    Bottom Layer, 0, 0, 0, 1192, 0, 0, 0, 0
    Mechanical 1, 0, 0, 0, 121, 1, 0, 0, 0
    Mechanical 13, 0, 0, 0, 3384, 0, 0, 0, 846
    Mechanical 15, 0, 0, 0, 5076, 0, 0, 0, 0
    Top Overlay, 179, 0, 0, 748, 1866, 0, 0, 0
    Bottom Overlay, 0, 0, 0, 0, 0, 0, 0, 0
    Top Paste, 0, 0, 0, 0, 0, 0, 0, 0
    Bottom Paste, 0, 0, 0, 0, 0, 0, 0, 0
    Top Solder, 0, 0, 0, 0, 0, 0, 0, 0
    Bottom Solder, 0, 0, 0, 0, 0, 0, 0, 0
    Drill Guide, 0, 0, 0, 0, 0, 0, 0, 0
    Keep-Out Layer, 0, 0, 0, 0, 0, 0, 0, 0
    Drill Drawing, 0, 0, 0, 0, 0, 0, 0, 0
    Multi-Layer, 0, 158, 464, 0, 0, 0, 0, 0
count : 19

Layer Pairs, Vias
    Top Layer - Bottom Layer, 464
count : 1

Non-Plated Hole Size, Pads, Vias
count : 0

Plated Hole Size, Pads, Vias
    0mils, 1871, 0
    19.7mils, 60, 0
    28mils, 0, 464
    39.37mils, 96, 0
    110.236mils, 2, 0
count : 5

Non-Plated Slot Size / Length, Pads
count : 0

Plated Slot Size / Length, Pads
count : 0

Non-Plated Square Hole Size, Pads
count : 0

Plated Square Hole Size, Pads
count : 0

Top Layer Annular Ring Size, Count
    20.3mils, 60
    22mils, 464
    22.63mils, 96
    70.866mils, 2
count : 4

Mid Layer Annular Ring Size, Count
    20.3mils, 60
    22mils, 464
    22.63mils, 96
    70.866mils, 2
count : 4

Bottom Layer Annular Ring Size, Count
    20.3mils, 60
    22mils, 464
    22.63mils, 96
    70.866mils, 2
count : 4

Pad Solder Mask, Count
    4mils, 2029
count : 1

Pad Paste Mask, Count
    0mils, 2029
count : 1

Pad Pwr/Gnd Expansion, Count
    20mils, 2029
count : 1

Pad Relief Conductor Width, Count
    10mils, 2029
count : 1

Pad Relief Air Gap, Count
    10mils, 2029
count : 1

Pad Relief Entries, Count
    4, 2029
count : 1

Via Solder Mask, Count
    4mils, 464
count : 1

Via Pwr/Gnd Expansion, Count
    20mils, 464
count : 1

Track Width, Count
    3.937mils, 8461
    5mils, 775
    5.086mils, 60
    7mils, 5162
    7.874mils, 663
    10mils, 40
    15mils, 7
    40mils, 12
count : 8

Arc Line Width, Count
    9.843mils, 159
    10mils, 20
count : 2

Arc Radius, Count
    4.921mils, 159
    18.868mils, 20
count : 2

Arc Degrees, Count
    360, 179
count : 1

Text Height, Count
    20mils, 198
    23.622mils, 1
    30mils, 55
    40mils, 1
    59.055mils, 7
    60mils, 1605
count : 6

Text Width, Count
    1.969mils, 1
    5.906mils, 7
    7mils, 248
    8mils, 6
    10mils, 1605
count : 5

Net Track Width, Count
    0mils, 1
    4mils, 30
    10mils, 453
count : 3

Net Via Size, Count
    50mils, 484
count : 1