customize

# Board Information Report

Date | : | 6/25/2009
Time | : | 1:39:32 PM
Elapsed Time | : | 00:00:00
Filename | : | C:\Documents and Settings\jonesrt\My Documents\Analog Board, Spring 2009\Amplifier Board.PcbDoc
Units | : | mmmils

## Contents

Contents

Board Specification

General

Routing

Routing Information

Layer Information

Layer Information

Layer Pairs

Board Holes

Non-Plated Hole Size

Plated Hole Size

Board Slots

Non-Plated Slot Size

Plated Slot Size

Board Square Holes

Non-Plated Square Hole Size

Plated Square Hole Size

Other

Top Layer Annular Ring Size

Mid Layer Annular Ring Size

Bottom Layer Annular Ring Size

Pad Solder Mask

Pad Paste Mask

Pad Pwr/Gnd Expansion

Pad Relief Conductor Width

Pad Relief Air Gap

Pad Relief Entries

Via Solder Mask

Via Pwr/Gnd Expansion

Track Width

Arc Line Width

Arc Radius

Arc Degrees

Text Height

Text Width

Net Track Width

Net Via Size

## Board Specification

General
Board Size | 6000mils x 2640mils
Components on board | 884

Back to top

## Routing

Routing Information
Routing completion | 100.00%
Connections | 1513
Connections routed | 1513
Connections remaing | 0

Back to top

## Layer Information

Layer | Arcs | Pads | Vias | Tracks | Texts | Fills | Regions | ComponentBodies
--- | --- | --- | --- | --- | --- | --- | --- | ---
Top Layer | 0 | 1871 | 0 | 4647 | 0 | 0 | 0 | 0
GND | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
VCC | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
BASES | 0 | 0 | 0 | 0 | 0 | 0 | 2 | 0
GND | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
Bottom Layer | 0 | 0 | 0 | 1192 | 0 | 0 | 0 | 0
Mechanical 1 | 0 | 0 | 0 | 121 | 1 | 0 | 0 | 0
Mechanical 13 | 0 | 0 | 0 | 3384 | 0 | 0 | 0 | 846
Mechanical 15 | 0 | 0 | 0 | 5076 | 0 | 0 | 0 | 0
Top Overlay | 179 | 0 | 0 | 748 | 1866 | 0 | 0 | 0
Bottom Overlay | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Top Paste | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Bottom Paste | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Top Solder | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Bottom Solder | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Drill Guide | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Keep-Out Layer | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Drill Drawing | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Multi-Layer | 0 | 158 | 464 | 0 | 0 | 0 | 0 | 0
Total | 179 | 2029 | 464 | 15180 | 1867 | 0 | 2 | 846

Back to top

Layer Pairs | Vias
--- | ---
Top Layer - Bottom Layer | 464
Total | 464

Back to top

## Board Holes

Non-Plated Hole Size | Pads | Vias
--- | --- | ---
Total | 0 | 0

Back to top

Plated Hole Size | Pads | Vias
--- | --- | ---
0mils | 1871 | 0
19.7mils | 60 | 0
28mils | 0 | 464
39.37mils | 96 | 0
110.236mils | 2 | 0
Total | 2029 | 464

Back to top

## Board Slots

Non-Plated Slot Size / Length | Pads
--- | ---
Total | 0

Back to top

Plated Slot Size / Length | Pads
--- | ---
Total | 0

Back to top

## Board Square Holes

Non-Plated Square Hole Size | Pads
--- | ---
Total | 0

Back to top

Plated Square Hole Size | Pads
--- | ---
Total | 0

Back to top

## Other

Top Layer Annular Ring Size | Count
--- | ---
20.3mils | 60
22mils | 464
22.63mils | 96
70.866mils | 2
Total | 622

Back to top

Mid Layer Annular Ring Size | Count
--- | ---
20.3mils | 60
22mils | 464
22.63mils | 96
70.866mils | 2
Total | 622

Back to top

Bottom Layer Annular Ring Size | Count
--- | ---
20.3mils | 60
22mils | 464
22.63mils | 96
70.866mils | 2
Total | 622

Back to top

Pad Solder Mask | Count
--- | ---
4mils | 2029
Total | 2029

Back to top

Pad Paste Mask | Count
--- | ---
0mils | 2029
Total | 2029

Back to top

Pad Pwr/Gnd Expansion | Count
--- | ---
20mils | 2029
Total | 2029

Back to top

Pad Relief Conductor Width | Count
--- | ---
10mils | 2029
Total | 2029

Back to top

Pad Relief Air Gap | Count
--- | ---
10mils | 2029
Total | 2029

Back to top

Pad Relief Entries | Count
--- | ---
4 | 2029
Total | 2029

Back to top

Via Solder Mask | Count
--- | ---
4mils | 464
Total | 464

Back to top

Via Pwr/Gnd Expansion | Count
--- | ---
20mils | 464
Total | 464

Back to top

Track Width | Count
--- | ---
3.937mils | 8461
5mils | 775
5.086mils | 60
7mils | 5162
7.874mils | 663
10mils | 40
15mils | 7
40mils | 12
Total | 15180

Back to top

Arc Line Width | Count
--- | ---
9.843mils | 159
10mils | 20
Total | 179

Back to top

Arc Radius | Count
--- | ---
4.921mils | 159
18.868mils | 20
Total | 179

Back to top

Arc Degrees | Count
--- | ---
360 | 179
Total | 179

Back to top

Text Height | Count
--- | ---
20mils | 198
23.622mils | 1
30mils | 55
40mils | 1
59.055mils | 7
60mils | 1605
Total | 1867

Back to top

Text Width | Count
--- | ---
1.969mils | 1
5.906mils | 7
7mils | 248
8mils | 6
10mils | 1605
Total | 1867

Back to top

Net Track Width | Count
--- | ---
0mils | 1
4mils | 30
10mils | 453
Total | 484

Back to top

Net Via Size | Count
--- | ---
50mils | 484
Total | 484

Back to top