Board Information Report
Filename     : C:\Documents and Settings\jonesrt\My Documents\GlueX\Prototype1.PcbDoc
Date         : 8/15/2008
Time         : 12:47:13 PM
Time Elapsed : 00:00:00

General
    Board Size, 2500.514milsx3790.509mils
    Components on board, 76
count : 2

Routing Information
    Routing completion, 100.00%
    Connections, 369
    Connections routed, 369
    Connections remaing, 0
count : 4

Layer, Arcs, Pads, Vias, Tracks, Texts, Fills, Regions, ComponentBodies
    Signal 1, 0, 447, 0, 1268, 0, 10, 0, 0
    DGND, 0, 0, 0, 4, 0, 0, 0, 0
    +3.3, 0, 0, 0, 4, 0, 0, 0, 0
    AGND, 0, 0, 0, 4, 0, 0, 0, 0
    +5/+1.2, 0, 0, 0, 0, 0, 0, 7, 0
    Signal 4, 0, 0, 0, 232, 0, 0, 0, 0
    Mechanical 1, 0, 0, 0, 3, 1, 0, 0, 0
    Mechanical 13, 3, 0, 0, 12, 0, 0, 0, 4
    Mechanical 15, 0, 0, 0, 23, 0, 0, 0, 0
    Top Overlay, 23, 0, 0, 195, 169, 0, 0, 0
    Bottom Overlay, 0, 0, 0, 0, 0, 0, 0, 0
    Top Paste, 0, 0, 0, 0, 0, 0, 0, 0
    Bottom Paste, 0, 0, 0, 0, 0, 0, 0, 0
    Top Solder, 0, 0, 0, 0, 0, 0, 0, 0
    Bottom Solder, 0, 0, 0, 0, 0, 0, 0, 0
    Drill Guide, 0, 0, 0, 0, 0, 0, 0, 0
    Keep-Out Layer, 0, 0, 0, 0, 0, 0, 0, 0
    Drill Drawing, 0, 0, 0, 0, 0, 0, 0, 0
    Multi-Layer, 0, 80, 161, 0, 0, 0, 0, 0
count : 19

Layer Pairs, Vias
    Signal 1 - Signal 4, 161
count : 1

Non-Plated Hole Size, Pads, Vias
    0mils, 160, 0
    127.953mils, 2, 0
count : 2

Plated Hole Size, Pads, Vias
    0mils, 287, 0
    12.992mils, 0, 9
    28mils, 0, 152
    35.433mils, 8, 0
    35.433mils, 18, 0
    39.37mils, 48, 0
    62.992mils, 2, 0
    110.236mils, 2, 0
count : 8

Non-Plated Slot Size / Length, Pads
count : 0

Plated Slot Size / Length, Pads
count : 0

Non-Plated Square Hole Size, Pads
count : 0

Plated Square Hole Size, Pads
count : 0

Top Layer Annular Ring Size, Count
    -11.811mils, 2
    12.992mils, 9
    22mils, 152
    22.63mils, 47
    23.622mils, 26
    25.591mils, 1
    41.339mils, 2
    70.866mils, 2
count : 8

Mid Layer Annular Ring Size, Count
    -11.811mils, 2
    12.992mils, 9
    22mils, 152
    22.63mils, 47
    23.622mils, 26
    25.591mils, 1
    41.339mils, 2
    70.866mils, 2
count : 8

Bottom Layer Annular Ring Size, Count
    -11.811mils, 2
    12.992mils, 9
    22mils, 152
    22.63mils, 47
    23.622mils, 26
    25.591mils, 1
    41.339mils, 2
    70.866mils, 2
count : 8

Pad Solder Mask, Count
    4mils, 527
count : 1

Pad Paste Mask, Count
    0mils, 527
count : 1

Pad Pwr/Gnd Expansion, Count
    20mils, 527
count : 1

Pad Relief Conductor Width, Count
    10mils, 527
count : 1

Pad Relief Air Gap, Count
    10mils, 527
count : 1

Pad Relief Entries, Count
    4, 527
count : 1

Via Solder Mask, Count
    4mils, 161
count : 1

Via Pwr/Gnd Expansion, Count
    20mils, 161
count : 1

Track Width, Count
    0.4mils, 22
    2mils, 3
    3mils, 12
    3.937mils, 38
    4mils, 231
    7.874mils, 173
    10mils, 1248
    20mils, 6
    40mils, 12
count : 9

Arc Line Width, Count
    0.4mils, 12
    3.937mils, 3
    7.874mils, 2
    9.843mils, 7
    23.622mils, 2
count : 5

Arc Radius, Count
    4.921mils, 7
    9.8mils, 4
    9.85mils, 8
    11.811mils, 3
    19.685mils, 3
    196.85mils, 1
count : 6

Arc Degrees, Count
    180, 13
    360, 13
count : 2

Text Height, Count
    23.622mils, 1
    30mils, 6
    40mils, 65
    50mils, 4
    59.055mils, 7
    60mils, 87
count : 6

Text Width, Count
    1.969mils, 1
    5.906mils, 7
    8mils, 10
    10mils, 152
count : 4

Net Track Width, Count
    4mils, 33
    10mils, 64
count : 2

Net Via Size, Count
    50mils, 97
count : 1