customize

# Board Information Report

Date | : | 8/20/2009
Time | : | 1:07:08 PM
Elapsed Time | : | 00:00:00
Filename | : | C:\Documents and Settings\jonesrt\My Documents\Backplane\Backplane_Tight.PcbDoc
Units | : | mmmils

## Contents

Contents

Board Specification

General

Routing

Routing Information

Layer Information

Layer Information

Layer Pairs

Board Holes

Non-Plated Hole Size

Plated Hole Size

Board Slots

Non-Plated Slot Size

Plated Slot Size

Board Square Holes

Non-Plated Square Hole Size

Plated Square Hole Size

Other

Top Layer Annular Ring Size

Mid Layer Annular Ring Size

Bottom Layer Annular Ring Size

Pad Solder Mask

Pad Paste Mask

Pad Pwr/Gnd Expansion

Pad Relief Conductor Width

Pad Relief Air Gap

Pad Relief Entries

Track Width

Text Height

Text Width

Net Track Width

Net Via Size

## Board Specification

General
Board Size | 6520mils x 1600mils
Components on board | 17

Back to top

## Routing

Routing Information
Routing completion | 100.00%
Connections | 116
Connections routed | 116
Connections remaing | 0

Back to top

## Layer Information

Layer | Arcs | Pads | Vias | Tracks | Texts | Fills | Regions | ComponentBodies
--- | --- | --- | --- | --- | --- | --- | --- | ---
Top Layer | 0 | 0 | 0 | 240 | 0 | 0 | 4 | 0
AGND | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
+5V | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
DGND | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
VCC | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
Bottom Layer | 0 | 0 | 0 | 219 | 0 | 0 | 0 | 0
Mechanical 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Top Overlay | 0 | 0 | 0 | 185 | 59 | 0 | 0 | 0
Bottom Overlay | 0 | 0 | 0 | 6 | 9 | 0 | 0 | 0
Top Paste | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Bottom Paste | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Top Solder | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Bottom Solder | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Drill Guide | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Keep-Out Layer | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Drill Drawing | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Multi-Layer | 0 | 229 | 0 | 0 | 0 | 0 | 0 | 0
Total | 0 | 229 | 0 | 666 | 68 | 0 | 4 | 0

Back to top

Layer Pairs | Vias
--- | ---
Total | 0

Back to top

## Board Holes

Non-Plated Hole Size | Pads | Vias
--- | --- | ---
Total | 0 | 0

Back to top

Plated Hole Size | Pads | Vias
--- | --- | ---
27.559mils | 55 | 0
35.433mils | 14 | 0
39.37mils | 144 | 0
47.244mils | 6 | 0
110.236mils | 4 | 0
138mils | 3 | 0
150mils | 3 | 0
Total | 229 | 0

Back to top

## Board Slots

Non-Plated Slot Size / Length | Pads
--- | ---
Total | 0

Back to top

Plated Slot Size / Length | Pads
--- | ---
Total | 0

Back to top

## Board Square Holes

Non-Plated Square Hole Size | Pads
--- | ---
Total | 0

Back to top

Plated Square Hole Size | Pads
--- | ---
Total | 0

Back to top

## Other

Top Layer Annular Ring Size | Count
--- | ---
19.756mils | 6
22.63mils | 144
23.622mils | 14
32.441mils | 55
70.866mils | 4
150mils | 3
172mils | 3
Total | 229

Back to top

Mid Layer Annular Ring Size | Count
--- | ---
19.756mils | 6
22.63mils | 144
23.622mils | 14
32.441mils | 55
70.866mils | 4
150mils | 3
172mils | 3
Total | 229

Back to top

Bottom Layer Annular Ring Size | Count
--- | ---
19.756mils | 6
22.63mils | 144
23.622mils | 14
32.441mils | 55
70.866mils | 4
150mils | 3
172mils | 3
Total | 229

Back to top

Pad Solder Mask | Count
--- | ---
4mils | 229
Total | 229

Back to top

Pad Paste Mask | Count
--- | ---
0mils | 229
Total | 229

Back to top

Pad Pwr/Gnd Expansion | Count
--- | ---
20mils | 229
Total | 229

Back to top

Pad Relief Conductor Width | Count
--- | ---
10mils | 229
Total | 229

Back to top

Pad Relief Air Gap | Count
--- | ---
10mils | 229
Total | 229

Back to top

Pad Relief Entries | Count
--- | ---
4 | 229
Total | 229

Back to top

Track Width | Count
--- | ---
5mils | 369
7mils | 67
7.874mils | 24
10mils | 189
40mils | 16
50mils | 1
Total | 666

Back to top

Text Height | Count
--- | ---
30mils | 7
50mils | 4
59.055mils | 13
60mils | 44
Total | 68

Back to top

Text Width | Count
--- | ---
5.906mils | 13
6mils | 9
7mils | 2
8mils | 9
10mils | 35
Total | 68

Back to top

Net Track Width | Count
--- | ---
5mils | 83
10mils | 1
Total | 84

Back to top

Net Via Size | Count
--- | ---
50mils | 84
Total | 84

Back to top