customize

# Board Information Report

Date | : | 8/15/2008
Time | : | 12:47:13 PM
Elapsed Time | : | 00:00:00
Filename | : | C:\Documents and Settings\jonesrt\My Documents\GlueX\Prototype1.PcbDoc
Units | : | mmmils

## Contents

Contents

Board Specification

General

Routing

Routing Information

Layer Information

Layer Information

Layer Pairs

Board Holes

Non-Plated Hole Size

Plated Hole Size

Board Slots

Non-Plated Slot Size

Plated Slot Size

Board Square Holes

Non-Plated Square Hole Size

Plated Square Hole Size

Other

Top Layer Annular Ring Size

Mid Layer Annular Ring Size

Bottom Layer Annular Ring Size

Pad Solder Mask

Pad Paste Mask

Pad Pwr/Gnd Expansion

Pad Relief Conductor Width

Pad Relief Air Gap

Pad Relief Entries

Via Solder Mask

Via Pwr/Gnd Expansion

Track Width

Arc Line Width

Arc Radius

Arc Degrees

Text Height

Text Width

Net Track Width

Net Via Size

## Board Specification

General
Board Size | 2500.514mils x 3790.509mils
Components on board | 76

Back to top

## Routing

Routing Information
Routing completion | 100.00%
Connections | 369
Connections routed | 369
Connections remaing | 0

Back to top

## Layer Information

Layer | Arcs | Pads | Vias | Tracks | Texts | Fills | Regions | ComponentBodies
--- | --- | --- | --- | --- | --- | --- | --- | ---
Signal 1 | 0 | 447 | 0 | 1268 | 0 | 10 | 0 | 0
DGND | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
+3.3 | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
AGND | 0 | 0 | 0 | 4 | 0 | 0 | 0 | 0
+5/+1.2 | 0 | 0 | 0 | 0 | 0 | 0 | 7 | 0
Signal 4 | 0 | 0 | 0 | 232 | 0 | 0 | 0 | 0
Mechanical 1 | 0 | 0 | 0 | 3 | 1 | 0 | 0 | 0
Mechanical 13 | 3 | 0 | 0 | 12 | 0 | 0 | 0 | 4
Mechanical 15 | 0 | 0 | 0 | 23 | 0 | 0 | 0 | 0
Top Overlay | 23 | 0 | 0 | 195 | 169 | 0 | 0 | 0
Bottom Overlay | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Top Paste | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Bottom Paste | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Top Solder | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Bottom Solder | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Drill Guide | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Keep-Out Layer | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Drill Drawing | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
Multi-Layer | 0 | 80 | 161 | 0 | 0 | 0 | 0 | 0
Total | 26 | 527 | 161 | 1745 | 170 | 10 | 7 | 4

Back to top

Layer Pairs | Vias
--- | ---
Signal 1 - Signal 4 | 161
Total | 161

Back to top

## Board Holes

Non-Plated Hole Size | Pads | Vias
--- | --- | ---
0mils | 160 | 0
127.953mils | 2 | 0
Total | 162 | 0

Back to top

Plated Hole Size | Pads | Vias
--- | --- | ---
0mils | 287 | 0
12.992mils | 0 | 9
28mils | 0 | 152
35.433mils | 8 | 0
35.433mils | 18 | 0
39.37mils | 48 | 0
62.992mils | 2 | 0
110.236mils | 2 | 0
Total | 365 | 161

Back to top

## Board Slots

Non-Plated Slot Size / Length | Pads
--- | ---
Total | 0

Back to top

Plated Slot Size / Length | Pads
--- | ---
Total | 0

Back to top

## Board Square Holes

Non-Plated Square Hole Size | Pads
--- | ---
Total | 0

Back to top

Plated Square Hole Size | Pads
--- | ---
Total | 0

Back to top

## Other

Top Layer Annular Ring Size | Count
--- | ---
-11.811mils | 2
12.992mils | 9
22mils | 152
22.63mils | 47
23.622mils | 26
25.591mils | 1
41.339mils | 2
70.866mils | 2
Total | 241

Back to top

Mid Layer Annular Ring Size | Count
--- | ---
-11.811mils | 2
12.992mils | 9
22mils | 152
22.63mils | 47
23.622mils | 26
25.591mils | 1
41.339mils | 2
70.866mils | 2
Total | 241

Back to top

Bottom Layer Annular Ring Size | Count
--- | ---
-11.811mils | 2
12.992mils | 9
22mils | 152
22.63mils | 47
23.622mils | 26
25.591mils | 1
41.339mils | 2
70.866mils | 2
Total | 241

Back to top

Pad Solder Mask | Count
--- | ---
4mils | 527
Total | 527

Back to top

Pad Paste Mask | Count
--- | ---
0mils | 527
Total | 527

Back to top

Pad Pwr/Gnd Expansion | Count
--- | ---
20mils | 527
Total | 527

Back to top

Pad Relief Conductor Width | Count
--- | ---
10mils | 527
Total | 527

Back to top

Pad Relief Air Gap | Count
--- | ---
10mils | 527
Total | 527

Back to top

Pad Relief Entries | Count
--- | ---
4 | 527
Total | 527

Back to top

Via Solder Mask | Count
--- | ---
4mils | 161
Total | 161

Back to top

Via Pwr/Gnd Expansion | Count
--- | ---
20mils | 161
Total | 161

Back to top

Track Width | Count
--- | ---
0.4mils | 22
2mils | 3
3mils | 12
3.937mils | 38
4mils | 231
7.874mils | 173
10mils | 1248
20mils | 6
40mils | 12
Total | 1745

Back to top

Arc Line Width | Count
--- | ---
0.4mils | 12
3.937mils | 3
7.874mils | 2
9.843mils | 7
23.622mils | 2
Total | 26

Back to top

Arc Radius | Count
--- | ---
4.921mils | 7
9.8mils | 4
9.85mils | 8
11.811mils | 3
19.685mils | 3
196.85mils | 1
Total | 26

Back to top

Arc Degrees | Count
--- | ---
180 | 13
360 | 13
Total | 26

Back to top

Text Height | Count
--- | ---
23.622mils | 1
30mils | 6
40mils | 65
50mils | 4
59.055mils | 7
60mils | 87
Total | 170

Back to top

Text Width | Count
--- | ---
1.969mils | 1
5.906mils | 7
8mils | 10
10mils | 152
Total | 170

Back to top

Net Track Width | Count
--- | ---
4mils | 33
10mils | 64
Total | 97

Back to top

Net Via Size | Count
--- | ---
50mils | 97
Total | 97

Back to top