Board Information Report
Filename     : C:\Documents and Settings\jonesrt\My Documents\Backplane\Backplane_Tight.PcbDoc
Date         : 11/12/2009
Time         : 1:09:52 PM
Time Elapsed : 00:00:00

General
    Board Size, 6940milsx1650mils
    Components on board, 21
count : 2

Routing Information
    Routing completion, 100.00%
    Connections, 126
    Connections routed, 126
    Connections remaing, 0
count : 4

Layer, Arcs, Pads, Vias, Tracks, Texts, Fills, Regions, ComponentBodies
    Top Layer, 0, 2, 0, 255, 0, 0, 4, 0
    AGND, 0, 0, 0, 4, 0, 0, 0, 0
    +5V, 0, 0, 0, 4, 0, 0, 0, 0
    DGND, 0, 0, 0, 4, 0, 0, 0, 0
    VCC, 0, 0, 0, 4, 0, 0, 0, 0
    Bottom Layer, 0, 0, 0, 234, 0, 0, 0, 0
    Mechanical 1, 0, 0, 0, 0, 0, 0, 0, 0
    Mechanical 13, 0, 0, 0, 4, 0, 0, 0, 1
    Mechanical 15, 0, 0, 0, 6, 0, 0, 0, 0
    Top Overlay, 0, 0, 0, 127, 66, 0, 0, 0
    Bottom Overlay, 0, 0, 0, 6, 9, 0, 0, 0
    Top Paste, 0, 0, 0, 0, 0, 0, 0, 0
    Bottom Paste, 0, 0, 0, 0, 0, 0, 0, 0
    Top Solder, 0, 0, 0, 0, 0, 0, 0, 0
    Bottom Solder, 0, 0, 0, 0, 0, 0, 0, 0
    Drill Guide, 0, 0, 0, 0, 0, 0, 0, 0
    Keep-Out Layer, 0, 0, 0, 0, 0, 0, 0, 0
    Drill Drawing, 0, 0, 0, 0, 0, 0, 0, 0
    Multi-Layer, 0, 241, 0, 0, 0, 0, 0, 0
count : 19

Layer Pairs, Vias
count : 0

Non-Plated Hole Size, Pads, Vias
count : 0

Plated Hole Size, Pads, Vias
    0mils, 2, 0
    27.559mils, 61, 0
    35.433mils, 20, 0
    39.37mils, 144, 0
    47.244mils, 6, 0
    110.236mils, 4, 0
    138mils, 6, 0
count : 7

Non-Plated Slot Size / Length, Pads
count : 0

Plated Slot Size / Length, Pads
count : 0

Non-Plated Square Hole Size, Pads
count : 0

Plated Square Hole Size, Pads
count : 0

Top Layer Annular Ring Size, Count
    19.685mils, 6
    19.756mils, 6
    22.63mils, 144
    23.622mils, 20
    32.441mils, 55
    70.866mils, 4
    172mils, 6
count : 7

Mid Layer Annular Ring Size, Count
    19.685mils, 6
    19.756mils, 6
    22.63mils, 144
    23.622mils, 20
    32.441mils, 55
    70.866mils, 4
    172mils, 6
count : 7

Bottom Layer Annular Ring Size, Count
    19.685mils, 6
    19.756mils, 6
    22.63mils, 144
    23.622mils, 20
    32.441mils, 55
    70.866mils, 4
    172mils, 6
count : 7

Pad Solder Mask, Count
    4mils, 243
count : 1

Pad Paste Mask, Count
    0mils, 243
count : 1

Pad Pwr/Gnd Expansion, Count
    20mils, 243
count : 1

Pad Relief Conductor Width, Count
    10mils, 243
count : 1

Pad Relief Air Gap, Count
    10mils, 243
count : 1

Pad Relief Entries, Count
    4, 243
count : 1

Track Width, Count
    3.937mils, 10
    5mils, 335
    7mils, 82
    7.874mils, 38
    10mils, 167
    40mils, 16
count : 6

Text Height, Count
    30mils, 7
    50mils, 4
    59.055mils, 13
    60mils, 51
count : 4

Text Width, Count
    5.906mils, 13
    7mils, 2
    8mils, 9
    10mils, 51
count : 4

Net Track Width, Count
    5mils, 90
    10mils, 1
count : 2

Net Via Size, Count
    50mils, 91
count : 1